{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":63,"n_cols":7,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[null,"In the functions below, btu is optional. If btu is set to true, both the arguments and the result"]
[null,"are in BTU. If btu is set to false or does not exist, both the arguments and the result are in SI."]
[]
[null,null,"Arguments for the functions and their units","UNIT in SI","UNIT in BTU"]
[null,"p  ","Pressure","kPa","psia"]
[null,"t  ","Temperature","°K","°F"]
[null,"h  ","Specific enthalpy","kJ/kg","Btu/lbm"]
[null,"s  ","Specific entropy","kJ/kg °K","Btu/lbm °F"]
[]
[]
[null,"Functions for saturated liquid and steam given pressure"]
[null,"s_tsat(p,btu)","Saturation temperature given pressure","°K","°F"]
[null,"s_vfp(p,btu)","Specific volume of saturated liquid","m3/kg","ft3/lbm"]
[null,"s_vgp(p,btu)","Specific volume of saturated steam","m3/kg","ft3/lbm"]
[null,"s_hfp(p,btu)","Specific enthalpy of saturated liquid","kJ/kg","Btu/lbm"]
[null,"s_hgp(p,btu)","Specific enthalpy of saturated steam","kJ/kg","Btu/lbm"]
[null,"s_sfp(p,btu)","Specific entropy of saturated liquid","kJ/kg °K","Btu/lbm °F"]
[null,"s_sgp(p,btu)","Specific entropy of saturated steam","kJ/kg °K","Btu/lbm °F"]
[null,"s_mufp(p,btu)","Dynamic viscosity of saturated liquid","Pa-s","lbf-s/ft2"]
[null,"s_mugp(p,btu)","Dynamic viscosity of saturated steam","kJ/kg °K","Btu/lbm °F"]
[null,"s_kfp(p,btu)","Thermal conductivity of saturated liquid","W/m °K","Btu/ft-hr-°F"]
[null,"s_kgp(p,btu)","Thermal conductivity of saturated steam","W/m °K","Btu/ft-hr-°F"]
[]
[null,"Functions for saturated liquid and steam given temperature"]
[null,"s_psat(t,btu)","Saturation pressure given temperature","kPa","psia"]
[null,"s_vft(t,btu)","Specific volume of saturated liquid","m3/kg","ft3/lbm"]
[null,"s_vgt(t,btu)","Specific volume of saturated steam","m3/kg","ft3/lbm"]
[null,"s_hft(t,btu)","Specific enthalpy of saturated liquid","kJ/kg","Btu/lbm"]
[null,"s_hgt(t,btu)","Specific enthalpy of saturated steam","kJ/kg","Btu/lbm"]
[null,"s_sft(t,btu)","Specific entropy of saturated liquid","kJ/kg °K","Btu/lbm °F"]
[null,"s_sgt(t,btu)","Specific entropy of saturated steam","kJ/kg °K","Btu/lbm °F"]
[null,"s_muft(t,btu)","Dynamic viscosity of saturated liquid","Pa-s","lbf-s/ft2"]
[null,"s_mugt(t,btu)","Dynamic viscosity of saturated steam","Pa-s","lbf-s/ft2"]
[null,"s_kft(t,btu)","Thermal conductivity of saturated liquid","W/m °K","Btu/ft-hr-°F"]
[null,"s_kgt(t,btu)","Thermal conductivity of saturated steam","W/m °K","Btu/ft-hr-°F"]
[]
[null,"Functions for non-saturated cases given pressure and temperature"]
[null,"s_vpt(p,t,btu)","Specific volume","m3/kg","ft3/lbm"]
[null,"s_hpt(p,t,btu)","Specific enthalpy","kJ/kg","Btu/lbm"]
[null,"s_spt(p,t,btu)","Specific entropy","kJ/kg °K","Btu/lbm °F"]
[null,"s_mupt(p,t,btu)","Dynamic viscosity","Pa-s","lbf-s/ft2"]
[null,"s_kpt(p,t,btu)","Thermal conductivity","W/m °K","Btu/ft-hr-°F"]
[null,"s_cppt(p,t,btu)","Specific heat at constant pressure","kJ/kg °K","Btu/lbm °F"]
[]
[null,"Temperature and quality given enthalpy (saturated or non-saturated)"]
[null,"s_tph(p,h,btu)","Temperature given pressure and enthalpy","°K","°F"]
[null,"s_xph(p,h,btu)","Quality given pressure and enthalpy","-","-"]
[]
[null,"Temperature and quality given entropy (saturated or non-saturated)"]
[null,"s_tps(p,s,btu)","Temperature given pressure and entropy","°K","°F"]
[null,"s_xps(p,s,btu)","Quality given pressure and entropy","-","-"]
[]
[]
[]
[null,null,null,"Sample calculations"]
[null,null,null,"Pressure","Temperature","Enthalpy","Entropy"]
[null,null,null,"kPa","°K","kJ/kg","kJ/kg-°K"]
[null,null,null,12000,400,{"$f":"s_hpt(D59,E59)","v":541.04527756986022},{"$f":"s_spt(D59,E59)","v":1.5902257051325612}]
[]
[null,null,null,"Pressure","Temperature","Enthalpy","Entropy"]
[null,null,null,"psia","°F","Btu/lbm","Btu/lbm °F"]
[null,null,null,1740.45,260.33,{"$f":"s_hpt(D63,E63,TRUE)","v":232.60761344270807},{"$f":"s_spt(D63,E63,TRUE)","v":0.37981891803023815}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}